Elantec
SUBCKT ELH0002/EL      In+ V1+ V2+ V1- V2- Out  <AutoShape>  [Misc]
SUBCKT ELH0032/EL      In+ In- V+ V- Q1=Comp Q2=Comp Q3=Comp Out  <Amplifier8> [OpAmp]
SUBCKT ELH0033/EL      In+ V+ Vc+ V- Vc- Out  <AutoShape>  [Misc]
SUBCKT ELH0101/EL      In+ In- V+ Q1=Isc+ Q2=Feedback V- Q3=Isc- Out  <Amplifier8>  [Misc]
SUBCKT buffer/EL       Unresolved pinout 7 terminals  [-]
SUBCKT lf156/EL        In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2001/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EL2002/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EL2003/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EL2004/EL       In+ V+ Vc+ V- Vc- Out  <AutoShape>  [Misc]
SUBCKT EL2005/EL       In+ V+ Vc+ V- Vc- Out  <AutoShape>  [Misc]
SUBCKT EL2006/EL       In+ In- V+ V- Q1=Comp Q2=Comp Q3=Comp Out  <Amplifier8> [OpAmp]
SUBCKT EL2008/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EL2009/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EL2012/EL       In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT EP2015/EL       q1c q1b q1e q2c q2b q2e q3c q3b q3e q4c q4b q4e  <AutoShape>  [Misc]
SUBCKT EN2016/EL       q1c q1b q1e q2c q2b q2e q3c q3b q3e q4c q4b q4e  <AutoShape>  [Misc]
SUBCKT EL2018/EL       In+ In- V+ V- Q1=~Le Q2=~Cs Out  <Amplifier7>  [Misc]
SUBCKT EL2019/EL       In+ In- V+ V- Q1=Cpin Q2=~Cs Out  <Amplifier7>  [Misc]
SUBCKT EL2020/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2022/EL       In+ In- V+ Q1=V+Coll V- Q2=V-Coll Out  <Amplifier7>  [Misc]
SUBCKT EL2028/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2029/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2030/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2038/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2039/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2040/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2041/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2044/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2045/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2070/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2071/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2073/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2074/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2075/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2082/EL       Vgain Iin Vin Iout  <AutoShape>  [Misc]
SUBCKT EL2090/EL       Vidin+ Vidin- V+ V- VidOut SHIn+ SHIn- SHOut HoldControl Chold  <AutoShape>  [Misc]
SUBCKT EL2099/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2120/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2160/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2176/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2186/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2190/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2210/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2211/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2223/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2224/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2232/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2242/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2243/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2244/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2245/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2252/EL       In+ In- V+ V- Q1=Hys Q2=~TTL Out  <Amplifier7>  [Misc]
SUBCKT EL2260/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2423/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2424/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2444/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2445/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2460/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2500/EL       In+ In- V+ V- Out Q=Comp  <Amplifier6> [OpAmp]
SUBCKT EL2520/EL       In+ In- V+ V- Out Q=Comp  <Amplifier6> [OpAmp]
SUBCKT EL2539/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2540/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL2600/EL       In+ In- V+ V- Out Q=Comp  <Amplifier6> [OpAmp]
SUBCKT EL2620/EL       In+ In- V+ V- Out Q=Comp  <Amplifier6> [OpAmp]
SUBCKT EL400/EL        In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL4083          Iz Ix Iy V- V+ Ixy Iyx  <AutoShape>  [Misc]
SUBCKT EL4089/EL       In- In+ Q1=Ref Q2=Hold V- Out V+  <Amplifier7>  [Misc]
SUBCKT EL4094/EL       InB Out ~Vgain Vgain InA  <AutoShape>  [Misc]
SUBCKT EL4095/EL       In+B In-B ~ForceA ~ForceB Out ~Vgain Vgain In-A In+A  <AutoShape>  [Misc]
SUBCKT EL4393/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT EL5190/EL       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT M7661           InA InB OutLA OutLB OutHA OutHB V-HA V-HB V-L V+HA V+HB V+L  <AutoShape>  [Misc]
SUBCKT comp10          Unresolved pinout 4 terminals  [-]
SUBCKT delay           Unresolved pinout 3 terminals  [-]
SUBCKT outstg          Unresolved pinout 5 terminals  [-]
