031 DIL*8   ( NC In- In+ V- NC Out V+); PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
1014 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
1230 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
124 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
2027 DIL*8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
2264 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4 );
2354 DIL*14 SO14 TSSOP14( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
33076 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- V-/2 NC In+/2 In-/2 Out/2 NC NC V-/3 V-/4 V+ NC Out);
404 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
412 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
471 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC In-/3 Out/3 In-/4 In+/3 V- In+/4 NC Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
6041 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
623 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
628 DIL*8 SO8 ( NC In- In+ V- NC Out NC V+);
6462 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC NC V-);
675 TO220 ( In+ In- V- Out V+);
747 DIL*14 ( In- In+ NC V- NC In+/2 In-/2 NC V+/2 Out/2 NC Out V+ NC);  PLCC20 ( NC In- In+ NC NC V- NC NC In+/2 In-/2 NC NC V+/2 Out/2 NC NC NC Out V+ NC);
772 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
798 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
804 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
812 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
814 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD584  DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD584J DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD584K DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD584L DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD584S DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD584T DIL*8   ( 10.0V 5.0V 2.5V Gnd Strobe VBG Cap Vin);
AD587 DIL*8 ( NC Vin NC Gnd Trim Out NC Noise);
AD587J DIL*8 ( NC Vin NC Gnd Trim Out NC Noise); SO8 ( NC Vin NC Gnd Trim Out NC Noise);
AD587K DIL*8 ( NC Vin NC Gnd Trim Out NC Noise);
AD587L DIL*8 ( NC Vin NC Gnd Trim Out NC Noise);
AD648A DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD648B DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD648C DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD680 DIL*8 SO8 ( NC Vin TEMP Gnd NC Out);
AD680JT TO92 ( Gnd Out Vin);
AD704 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
AD704A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD704J DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD704K DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD706 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD706A SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD706J DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD706K DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD711J DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD711K DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD712J DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD712K DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD713  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD713J DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD713K DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
AD743 DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+);
AD743A DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+);
AD743J DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+);
AD743K DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+);
AD745 DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+);
AD745A ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+); DIL*8 ( NC In- In+ V- NC Out V+);
AD745J SO16 ( NC NC In- NC In+ V- NC NC NC NC NC Out V+); DIL*8 ( NC In- In+ V- NC Out V+);
AD745K DIL*8 ( NC In- In+ V- NC Out V+);
AD746J DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD8001A DIL*8 ( NC In- In+ V- NC Out V+); SO8 ( NC In- In+ V- NC Out V+);
AD8001AN DIL*8 ( NC In- In+ V- NC Out V+);
AD8001AR SO8 ( NC In- In+ V- NC Out V+);
AD811 DIL*8 SO8 ( NC In- In+ V- NC Out V+); DIL*16 ( NC NC In- NC In+ NC V- NC NC NC NC Out NC V+); DIL*20 ( NC NC NC In- NC In+ NC V- NC NC NC NC NC NC Out NC V+);  PLCC20 ( NC NC NC NC NC In- NC In+ V- NC NC NC NC Out NC V+);
AD812 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD812A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD817 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD817A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD818 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD818A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD820 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
AD824 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD824A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD824B DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD826 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD826A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD828 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD828A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AD829 DIL*8  SO8 ( NC In- In+ V- Comp Out V+ NC);
AD829J DIL*8 SO8 ( NC In- In+ V- Comp Out V+ NC);
AD845 DIL*8 ( NC In- In+ V- NC Out V+ NC); SO16 ( NC NC NC In- In+ V- NC NC NC NC NC Out V+ NC);
AD845J DIL*8 ( NC In- In+ V- NC Out V+ NC); SO16 ( NC NC NC In- In+ V- NC NC NC NC NC Out V+ NC);
AD845K DIL*8 ( NC In- In+ V- NC Out V+ NC);
AD847 DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
AD847J DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
AD848 DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
AD848J DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
AN4558 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AN6552 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AN6553 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
AN6554 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
BUF04 DIL*8 SO8  ( NC NC In+ V- NC Out V+);
BUF600X1 DIL*8 SO8 ( V+ NC NC In+ V- NC NC Out);
BUF600X2 DIL*8 SO8 ( V+ NC NC In+ V- NC NC Out);
BUF601X1 DIL*8 ( V+ NC NC In+ V- NC NC Out);
BUF601X2 DIL*8 SO8 ( V+ NC NC In+ V- NC NC Out);
CLC109 SO8 DIL*8 ( V+ NC NC In+ V- NC NC Out);
CLC111 SO8 DIL*8 ( V+ NC NC In+ V- NC NC Out);
CLC401 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC402 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC404 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC406 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC409 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC412 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
CLC414 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
CLC415 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
CLC420 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC428 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
CLC432 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
CLC440 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
CLC449 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2001 DIL*8 ( V+ In+ NC V- NC NC Out); SO20W ( NC V+ NC In+ NC NC NC V- NC NC NC NC NC NC NC NC Out);
EL2002 DIL*8 ( V+ In+ NC V- NC NC Out); SO20W ( NC V+ NC In+ NC NC NC V- NC NC NC NC NC NC NC NC Out);
EL2003 DIL*8 ( V+ In+ NC V- NC NC Out); SO20W ( NC V+ NC In+ NC NC NC V- NC NC NC NC NC NC NC NC Out);
EL2008 TO220 ( V- Out NC In+ V+);
EL2009 TO220 ( V- Out NC In+ V+);
EL2030 DIL*8 ( NC In- In+ V- NC Out V+); SO20W ( NC NC NC In- NC In+ NC V- NC NC NC NC NC NC Out NC V+);
EL2038 DIL*14 ( In+ NC V- NC NC NC NC Out NC V+ NC NC NC In-);
EL2039 DIL*14 ( In+ NC V- NC NC NC NC Out NC V+ NC NC NC In-);
EL2040 DIL*14 ( NC NC NC In- In+ V- NC NC NC Out V+);
EL2044 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2045 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2071 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2073 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2074 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2075 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2160 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
EL2210 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
EL2211 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
EL2224 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO20W ( NC NC NC Out NC In- In+ NC NC V- NC NC NC In+/2 In-/2 NC Out/2 NC NC V+);
EL2232 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16W ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
EL2242 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO20W ( NC NC NC Out In- In+ V- NC NC NC NC NC NC In+/2 In-/2 Out/2 V+);
EL2243 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO20W ( NC NC NC Out In- In+ V- NC NC NC NC NC NC In+/2 In-/2 Out/2 V+);
EL2244 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
EL2245 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
EL2260 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
EL2410 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
EL2411 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
EL2424 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO20W ( Out In- NC In+ NC V+ In+/2 NC In-/2 Out/2 Out/3 In-/3 NC In+/3 V- NC In+/4 NC In-/4 Out/4);
EL2444 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
EL2445 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
EL2460 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
HA17082 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
HA17084 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
HA17558 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
HA-5154 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
LF353 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LF412 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LF412A  DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LF442 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LF442A DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LF444 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LF444A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LF453 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM124 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LM124A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LM139 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);  PLCC20 ( NC Out Out/2 V+ NC In-/2 NC In+/2 In- In+ NC In-/3 In+/3 In-/4 NC In+/4 NC V- Out/4 Out/3);
LM158 DIL*8  SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM193 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM224 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LM239 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);  PLCC20 ( NC Out Out/2 V+ NC In-/2 NC In+/2 In- In+ NC In-/3 In+/3 In-/4 NC In+/4 NC V- Out/4 Out/3);
LM258 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM2902 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LM2904 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM293 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM324 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LM3302 DIL*14 ( Out/2 Out V+ In- In+ In-/2 In+/2 In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
LM339 DIL*14 ( Out/2 Out V+ In- In+ In-/2 In+/2 In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);  PLCC20 ( NC Out Out/2 V+ NC In-/2 NC In+/2 In- In+ NC In-/3 In+/3 In-/4 NC In+/4 NC V- Out/4 Out/3);
LM358 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM393 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM6118 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LM6142 DIL*8 SO8 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC NC V-);
LM6181 DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC In- In+ V- NC NC NC NC NC Out V+);
LM6218 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);( NC Out NC In- In+ NC V- NC In+/2 In-/2 NC Out/2 NC V+);
LM7131 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LM833 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6001 DIL*8   ( NC In- In+ V- NC Out V+);
LMC6001A DIL*8   ( NC In- In+ V- NC Out V+);
LMC6022 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6024 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6032 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6034 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6041 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6041A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6042 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6042A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6044 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6044A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6061 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6061A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6062 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6062A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6064 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6064A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6081 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6081A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LMC6082 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6082A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6084 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6084A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6462 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6464 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6482A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6484A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6492 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6494 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC6582 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC6584 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC660 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC660A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LMC662 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC662A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LMC7101 DIL*8 ( NC In- In+ V- NC Out V+);
LP239/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
LP2901/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
LP339/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
LPC660 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LPC660A DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LPC661 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LPC661A DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LPC662 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LPC662A DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1013  DIL*8  ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1013D DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1014D DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1057S SO16W ( NC NC Out In- In+ V- NC NC NC NC In+/2 In-/2 Out/2 V+);
LT1058  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1058A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1078  DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1078A DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1079 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1079A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1178 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1178A DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1179 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1179A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1201 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1202 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1208 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1209 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1211 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1212 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1213 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1214 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1215 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1216 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1229 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1230 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1252 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LT1253 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1254 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1355 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1356 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1358 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1359 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1361 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1362 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LT1364 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
LT1365 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
LTC1047 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16W ( NC NC Out In- In+ V- NC NC NC NC In+/2 In-/2 Out/2 V+);
LTC1049 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
LTC1051 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16W ( NC NC Out In- In+ V- NC NC NC NC In+/2 In-/2 Out/2 V+);
LTC1053 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
M5216 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
M5220 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
M5228 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
M5238 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
M5260 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MB3607 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MB47082 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);   ( V+/2 Out In- In+ V- In+/2 In-/2 Out/2 V+);
MB47358 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);   ( V+/2 Out In- In+ V- In+/2 In-/2 Out/2 V+);
MB47833 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);   ( V+ Out In- In+ V- In+/2 In-/2 Out/2 V+/2);
MC1458 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC1458C DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC1458S DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC1558 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC1558S DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33072 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33074 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33076 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- V-/2 NC In+/2 In-/2 Out/2 NC NC V-/3 V-/4 V+ NC Out);
MC33078 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33079 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33172 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33174 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33178 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33179 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33182 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33184 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33272 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33274 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC33282 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
MC33284 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
MC34084 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16W ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-113 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-176 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-176G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-177 DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
OP-177F DIL*8 ( NC In- In+ V- NC Out V+ NC);
OP-177G DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
OP-183 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP191 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP191G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-200 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
OP-200G DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
OP-215 SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC In- In+ NC NC V- NC NC In+/2 In-/2 NC NC NC Out/2 NC NC NC Out V+);
OP-215E DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-215F DIL*8( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-215G SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-220 SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-220G SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-221G SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-249 SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
OP-249G SO8 ( In+ V- In+/2 In-/2 Out/2 V+ Out In-); DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-275 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-275G DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP279 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP279G DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-27E DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-27F DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-27G DIL*8 SO8   ( NC In- In+ V- NC Out V+ NC);
OP-282 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-282G DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-283 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP284 DIL*8 ( NC In- In+ V- NC Out V+);
OP284E DIL*8 ( NC In- In+ V- NC Out V+);
OP284F DIL*8 ( NC In- In+ V- NC Out V+);
OP-285 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-285G DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-290 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
OP-290G DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); SO16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
OP-291 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-292 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-295 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-297 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
OP-297F DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-297G DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OP-37 DIL*8 SO8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
OP-37E DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-37F DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-37G DIL*8 SO8   ( NC In- In+ V- NC Out V+ NC);
OP-400  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
OP-400G DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-400H DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-41 DIL*8 SO8   ( NC In- In+ V- NC Out V+);
OP-413 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16W ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-41G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-42 DIL*8 SO8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
OP-420  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
OP-420G  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-420H  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-421  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-421G  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-421H  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-42G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-43 DIL*8   ( NC In- In+ V- NC Out V+);
OP-43G DIL*8 ( NC In- In+ V- NC Out V+);
OP-44 DIL*8 SO8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
OP-467  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
OP-467G DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-470  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
OP471A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
OP-471A DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
OP471E DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-471E DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP471F DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-471F DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP471G DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC In-/3 Out/3 In-/4 In+/3 V- In+/4 NC Out/4);
OP-471G DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC In-/3 Out/3 In-/4 In+/3 V- In+/4 NC Out/4);
OP-482 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
OP-482G DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-490  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC28 ( NC Out In- NC NC In+ NC V+ NC In+/2 NC NC In-/2 Out/2 NC Out/3 In-/3 NC NC In+/3 NC V- NC In+/4 NC NC In-/4 Out/4);
OP-490G DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-491 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-492 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-497  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
OP-497F  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-497G  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OP-61 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
OP-77 DIL*8 SO8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
OP-77E DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-77F DIL*8   ( NC In- In+ V- NC Out V+ NC);
OP-77G DIL*8 SO8 ( NC In- In+ V- NC Out V+ NC);
OP-80 DIL*8 SO8   ( NC In- In+ V- NC Out V+);
OP-80G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OP-90 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
OP-90G DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA1013 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA1013E DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA124 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA124E DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA2107 DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2107E DIL*8 SO8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2111 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2111E DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2131 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2131E DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2604 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2604E DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2604M DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
OPA2658X DIL*8 SO8 ( NC In- In+ NC V- Out V+);
OPA404  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OPA404E  DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OPA4131 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OPA4131E SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OPA4658X DIL*16 SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
OPA603X DIL*8 ( NC In- In+ V- NC Out V+); SO16 ( NC NC In- NC In+ NC V- NC NC NC NC Out NC V+);
OPA620 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA620E DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA620X DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA621 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA621E DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA621X DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA623X1 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA623X2 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA648 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA650X DIL*8 SO8 ( NC In- In+ V- NC Out V+);
OPA658X DIL*8 SO8 ( NC In- In+ V- NC Out V+);
REF01 DIL*8   ( NC Vin NC Gnd Trim Out);  PLCC20 ( NC NC NC NC Vin NC NC NC NC Gnd NC Trim NC NC Out);
REF01A DIL*8   ( NC Vin NC Gnd Trim Out);
REF-01C DIL*8 SO8   ( NC Vin NC Gnd Trim Out);
REF01C DIL*8   ( NC Vin NC Gnd Trim Out);
REF01E DIL*8   ( NC Vin NC Gnd Trim Out);
REF-01H DIL*8   ( NC Vin NC Gnd Trim Out);
REF01H DIL*8   ( NC Vin NC Gnd Trim Out);
SSM-2131 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
SSM-2135 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75062P DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75064P DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TA75072P DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75074P DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TA75358P DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75458P DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75557P DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75558P DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TA75559P DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TL031/101 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL031/301 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL032/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL032/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL034/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL034/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL051/101 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL051/301 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL052/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL052/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL054/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL054/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL061/301 DIL*8 SO8 ( NC In- In+ V- NC Out V+);
TL062 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TL062/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TL064 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TL064/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL071/301 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL072/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL074/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TL081/301 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TL082 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TL082/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TL084 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TL084/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC1078/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC1078/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC1078/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC1078/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC1079/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC1079/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC1079/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC1079/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC2201/101 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLC2201/102 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLC2201/5_1 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLC2201/5_2 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLC2252 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2254 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC2262 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2262/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2262/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2262/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2262/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2264 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC2272/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2272/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2272/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2272/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC2274 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC252C/1_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC252C/1_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC252C/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC252C/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC254C/1_1 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC254C/1_2 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC254C/101 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC254C/102 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25L2C/1_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25L2C/1_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25L2C/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25L2C/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25L4C/1_1 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25L4C/1_2 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25L4C/101 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25L4C/102 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25M2C/1_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25M2C/1_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25M2C/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25M2C/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLC25M4C/1_1 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25M4C/1_2 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25M4C/101 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC25M4C/102 DIL*14 SO14   ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLC272/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC272/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC272/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC272/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC274/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC274/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC274/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC274/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC277/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC277/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC277/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC277/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC279/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC279/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC279/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC279/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L2/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L2/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L2/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L2/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L4/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L4/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L4/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L4/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L7/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L7/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L7/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L7/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27L9/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L9/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L9/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27L9/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M2/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M2/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M2/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M2/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M4/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M4/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M4/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M4/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M7/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M7/102 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M7/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M7/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC27M9/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M9/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M9/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC27M9/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLC339/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
TLC352/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC354/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
TLC3702/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLC3704/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);  PLCC20 ( NC Out Out/2 V+ NC In-/2 NC In+/2 In- In+ NC In-/3 In+/3 In-/4 NC In+/4 NC V- Out/4 Out/3);
TLC372/5_1 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);   DIL*8 ( V- In- In+ V- In+/2 In-/2 Out/2 V+ );
TLC374/5_1 DIL*14 ( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);  PLCC20 ( NC Out Out/2 V+ NC In-/2 NC In+/2 In- In+ NC In-/3 In+/3 In-/4 NC In+/4 NC V- Out/4 Out/3);
TLC393/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2021/301 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2021/302 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2021/5_1 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2021/5_2 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2022/301 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2022/302 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2022/5_1 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2022/5_2 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2024/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2024/302 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2024/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2024/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2027/301 DIL*8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
TLE2027/302 DIL*8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
TLE2037/301 DIL*8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
TLE2037/302 DIL*8   ( NC In- In+ V- NC Out V+ NC);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+ NC NC NC);
TLE2061/101 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2061/102 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2061/301 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2061/302 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2061/401 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2061/402 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2062/101 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2062/102 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2062/301 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2062/302 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2062/401 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2062/402 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2064/101 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2064/102 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2064/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2064/302 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2064/401 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2064/402 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2071 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2072 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2072/301 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2074 DIL*14  ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( Out NC In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2081 DIL*8 SO8 ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2082 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2082/101 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2084 DIL*14  ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); SO16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2141/301 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2141/302 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2141/5_1 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2141/5_2 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2142/301 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2142/302 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2142/5_1 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2142/5_2 DIL*8   ( Out In- In+ V- In+/2 In-/2 Out/2 V+);  PLCC20 ( NC Out NC NC In- NC In+ NC NC V- NC In+/2 NC NC In-/2 NC Out/2 NC NC V+);
TLE2144/301 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2144/302 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2144/5_1 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2144/5_2 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4); DIL*16 ( Out In- In+ V+ In+/2 In-/2 Out/2 NC NC Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);  PLCC20 ( NC Out In- In+ NC V+ NC In+/2 In-/2 Out/2 NC Out/3 In-/3 In+/3 NC V- NC In+/4 In-/4 Out/4);
TLE2161/101 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2161/102 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2161/301 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2161/302 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2161/401 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2161/402 DIL*8   ( NC In- In+ V- NC Out V+);  PLCC20 ( NC NC NC NC In- NC In+ NC NC V- NC NC NC NC Out NC V+);
TLE2227/301 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
TLE2227/302 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
TLE2237/301 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
TLE2237/302 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+); DIL*16 ( In- In+ NC V- NC In+/2 In-/2 NC NC Out/2 NC NC V+ NC NC Out);
TLV2252 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2254 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2262/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2262/3_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2262/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2262/5_2 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2263/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2264 DIL*14 SO14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2322I/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2322I/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2324I/3_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2324I/5_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2332I/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2332I/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2334I/3_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2334I/5_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2342I/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2342I/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2344I/3_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2344I/5_1 DIL*14 SO14 TSSOP14( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
TLV2352I/3_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2352I/5_1 DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
TLV2354I/3_1 DIL*14 SO14 TSSOP14( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
TLV2354I/5_1 DIL*14 SO14 TSSOP14( Out Out/2 V+ In-/2 In+/2 In- In+ In-/3 In+/3 In-/4 In+/4 V- Out/4 Out/3);
UA772 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
UA772A DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
UA772L DIL*8 SO8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
UA798 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC258 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC259 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4064 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC4074 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC4082 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4556 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4557 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4558 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4559 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4560 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC4570 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);   ( V+ Out In- In+ V- In+/2 In-/2 Out/2 V+/2);
uPC4572 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);   ( V+ Out In- In+ V- In+/2 In-/2 Out/2 V+/2);
uPC4574 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC458 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC4741 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC803 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC804 DIL*14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC812 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC814 DIL*8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC822 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC824 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC832 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC834 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
uPC842 DIL*8 SOP8 ( Out In- In+ V- In+/2 In-/2 Out/2 V+);
uPC844 DIL*14 SOP14 ( Out In- In+ V+ In+/2 In-/2 Out/2 Out/3 In-/3 In+/3 V- In+/4 In-/4 Out/4);
FZT705 TO92 ( B C E );
LF347 DIL*14 ( In- In+ Out V- V+ );
AD603 DIL*16 ( Com Feedback G- G+ In+ Out V- V+ );
ADG411 DIL*16 ( D1 D2 D3 );
