Burr-Brown
SUBCKT ACF2101M/BB     Com SwitchIn In+ Cap Out SwitchOut SwitchCom Reset Hold Select V+ V- Gnd  <AutoShape>  [Misc]
SUBCKT BUF600X1/BB     V+ In+ V- Out <Buffer4> [Buffer]
SUBCKT BUF600X2/BB     V+ In+ V- Out <Buffer4> [Buffer]
SUBCKT BUF601X1/BB     V+ In+ V- Out <Buffer4> [Buffer]
SUBCKT BUF601X2/BB     V+ In+ V- Out <Buffer4> [Buffer]
SUBCKT BUF634X/BB      In+ V+ V- Out <Buffer4> [Buffer]
SUBCKT INA101/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSet1 Q3=GainSet2  <Amplifier8> [InstAmp]
SUBCKT A1_101/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_101/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_101/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA101E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_101E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_101E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_101E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA102/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSet1 Q3=GainSet2  <Amplifier8> [InstAmp]
SUBCKT A1_102/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_102/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_102/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA102E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSet1 Q3=GainSet2  <Amplifier8> [InstAmp]
SUBCKT A1_102E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_102E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_102E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA103/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_103/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_103/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_103/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA103E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_103E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_103E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_103E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA105/BB       In+ In- V+ V- Out Q1=Ref Q2=Sense  <Amplifier7> [InstAmp]
SUBCKT A3_105/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA105E/BB      In+ In- V+ V- Out Q1=Ref Q2=Sense  <Amplifier7> [InstAmp]
SUBCKT A3_105E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA106/BB       In+ In- V+ V- Out Q1=Ref Q2=Sense  <Amplifier7> [InstAmp]
SUBCKT A3_106/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA106E/BB      In+ In- V+ V- Out Q1=Ref Q2=Sense  <Amplifier7> [InstAmp]
SUBCKT A3_106E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA110/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_110/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_110/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_110/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA110E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_110E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_110E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_110E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA111/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_111/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_111/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_111/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA111E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_111E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_111E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_111E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA114/BB       In+ In- V+ V- Out Q1=Feedback Q2=Ref Q3=GainSet1 Q4=GainSet2  <Amplifier9> [InstAmp]
SUBCKT A1_114/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_114/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_114/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA114E/BB      In+ In- V+ V- Out Q1=Feedback Q2=Ref Q3=GainSet1 Q4=GainSet2  <Amplifier9> [InstAmp]
SUBCKT A1_114E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_114E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_114E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA115/BB       In+ In- V+ V- Out Feedback Ref GainSet1 GainSet2 GainSense1 GainSense2  <AutoShape>  [InstAmp]
SUBCKT A1_115/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_115/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA115E/BB      In+ In- V+ V- Out Feedback Ref GainSet1 GainSet2 GainSense1 GainSense2  <AutoShape>  [InstAmp]
SUBCKT A1_115E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_115E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA117/BB       In+ In- V+ V- Out RefA RefB  <AutoShape>  [InstAmp]
SUBCKT A3_117/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA117E/BB      In+ In- V+ V- Out RefA RefB  <AutoShape>  [InstAmp]
SUBCKT A3_117E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA118/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_118/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_118/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_118/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA118E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_118E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_118E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_118E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA120/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_120/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_120/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_120/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA120E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSense1 Q3=GainSense2  <Amplifier8> [InstAmp]
SUBCKT A1_120E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A2_120E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_120E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA131/BB       In+ In- V+ V- Out Q1=Ref Q2=GainSet1 Q3=GainSet2  <Amplifier8> [InstAmp]
SUBCKT A1_131/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_131/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT INA131E/BB      In+ In- V+ V- Out Q1=Ref Q2=GainSet1 Q3=GainSet2  <Amplifier8> [InstAmp]
SUBCKT A1_131E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT A3_131E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT ISO120X/BB      +WS1 -WS1 Com2 Out VoutSense Gnd2 C2H C2L +WS2 -WS2 Com1 Vin Gnd1  <AutoShape>  [Misc]
SUBCKT ISO121X/BB      +WS1 -WS1 Com2 Out VoutSense Gnd2 C2H C2L +WS2 -WS2 Com1 Vin Gnd1  <AutoShape>  [Misc]
SUBCKT ISO130X/BB      VS1 In+ In- Gnd1 Gnd2 Out- Out+ VS2  <AutoShape>  [Misc]
SUBCKT IVC102M/BB      AGnd SwitchIn In- C1 C2 C3 V- Out Hold Reset DigGnd V+  <AutoShape>  [Misc]
SUBCKT OPA/BB          In- In+ Out V- V+  <Amplifier5> [OpAmp]
SUBCKT LOG100M/BB      In1 K-1 K-3 K-5 V+ Out V- Com In2  <AutoShape>  [Misc]
SUBCKT OPA1/BB         Unresolved pinout 6 terminals  [-]
SUBCKT OPA2/BB         Unresolved pinout 5 terminals  [-]
SUBCKT MPC100X1/BB     In1 In2 In3 In4 Sel4 Sel3 V+ Out V- Sel2 Sel1  <AutoShape>  [Misc]
SUBCKT MUX1/BB         In+ V- Out V+ Select  <AutoShape>  [Misc]
SUBCKT MPC100X2/BB     In1 In2 In3 In4 Sel4 Sel3 V+ Out V- Sel2 Sel1  <AutoShape>  [Misc]
SUBCKT MUX2/BB         In+ V- Out V+ Select  <AutoShape>  [Misc]
SUBCKT MPC102X1/BB     In1 In2 V+ In3 In4 Sel4 Sel3 Out1 V- Out2 Sel2 Sel1  <AutoShape>  [Misc]
SUBCKT MUX1/BB_R_1     Out1 In+ V- Out2 V+ <AutoShape> [Misc]
SUBCKT MPC104X1/BB     In1 V+ In2 Sel2 Out V- Sel1  <AutoShape>  [Misc]
SUBCKT MUX1/BB_R_2     Out1 In+ V- Out2 V+ <AutoShape> [Misc]
SUBCKT OPA101/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA1013/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA1013E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA101E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA102/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA102E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA111/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA111E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA121/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA121E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA124/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA124E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA128/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA128E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA129/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA129E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA130/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA131/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA131E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA132/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA134/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA177/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA177E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2107/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2107E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2111/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2111E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2130/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2131/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2131E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2132/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2234/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2234E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA234/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA234E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT opa237/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2541/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2541E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2544/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2604/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2604E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2604M/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA2658X/BB     In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA27/BB        In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA27E/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA27H/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA27HE/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA27M/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA37/BB        In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA37E/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA404/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA404E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4130/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4131/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4131E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4132/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4234/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4234E/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA445/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA445E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA4658X/BB     In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA501/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA501E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA502/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA502E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA511/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA511E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA512/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA512E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA541/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA541E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA544/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA602/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA602E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA603X/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT XN4LC/BB        Unresolved pinout 4 terminals  [-]
SUBCKT XN16HC/BB       Unresolved pinout 4 terminals  [-]
SUBCKT XP4LC/BB        Unresolved pinout 4 terminals  [-]
SUBCKT XP16HC/BB       Unresolved pinout 4 terminals  [-]
SUBCKT OPA604/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA604E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA604M/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA606/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA606E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA620/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA620E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA620X/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA621/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA621E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA621X/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA622X1/BB     IqAdj In- In+ V- OutV- Buff- Out OTA OutV+ V+ Buff+  <AutoShape>  [OpAmp]
SUBCKT DB/BB           Unresolved pinout 6 terminals  [-]
SUBCKT DT/BB           Unresolved pinout 9 terminals  [-]
SUBCKT CB/BB           Unresolved pinout 5 terminals  [-]
SUBCKT BC/BB           Unresolved pinout 5 terminals  [-]
SUBCKT OPA622X2/BB     IqAdj In- In+ V- OutV- Buff- Out OTA OutV+ V+ Buff+  <AutoShape>  [OpAmp]
SUBCKT DB/BB_R_1       Unresolved pinout 6 terminals  [-]
SUBCKT DT/BB_R_1       Unresolved pinout 9 terminals  [-]
SUBCKT CB/BB_R_1       Unresolved pinout 5 terminals  [-]
SUBCKT BC/BB_R_1       Unresolved pinout 5 terminals  [-]
SUBCKT OPA623X1/BB     In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT DT/BB_R_2       Unresolved pinout 8 terminals  [-]
SUBCKT CB/BB_R_2       Unresolved pinout 5 terminals  [-]
SUBCKT BC/BB_R_2       Unresolved pinout 4 terminals  [-]
SUBCKT OPA623X2/BB     In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT DT/BB_R_3       Unresolved pinout 8 terminals  [-]
SUBCKT CB/BB_R_3       Unresolved pinout 5 terminals  [-]
SUBCKT BC/BB_R_3       Unresolved pinout 4 terminals  [-]
SUBCKT OPA627/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA627E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA628M/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA637/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA637E/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA640X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA641X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA642X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA643X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA644X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA646X/BB      In- In+ V- Q1=OutV- Out V+ Q2=OutV+  <Amplifier7> [OpAmp]
SUBCKT OPA648X/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA650X/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA651M/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA651X/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA655M/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA658X/BB      In- In+ V- Out V+  <Amplifier5> [OpAmp]
SUBCKT OPA660X1/BB     IqAdj E B V- BuffInp BuffOut V+ C  <AutoShape>  [Misc]
SUBCKT MDB/BB          Unresolved pinout 6 terminals  [-]
SUBCKT MDT/BB          Unresolved pinout 7 terminals  [-]
SUBCKT MBC/BB          Unresolved pinout 5 terminals  [-]
SUBCKT OPA660X2/BB     IqAdj E B V- BuffInp BuffOut V+ C  <AutoShape>  [Misc]
SUBCKT MDB/BB_R_1      Unresolved pinout 6 terminals  [-]
SUBCKT MDT/BB_R_1      Unresolved pinout 7 terminals  [-]
SUBCKT MBC/BB_R_1      Unresolved pinout 5 terminals  [-]
SUBCKT OPA671M/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA675M         In+A In-A Comp Out V+ V- In+B In- Ecl ~ECL Gnd  <AutoShape>  [Misc]
OPA676M        In+A In-A Comp Out V+ V- In+B In- ~TTL Gnd  <AutoShape>  [Misc]
SUBCKT OPA77/BB        In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA77E/BB       In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT OPA350/BB       In+ In- V+ V- Out  <Amplifier5>  [OpAmp]                           
SUBCKT OPT101/BB       V+ In- VPD Feedback Out Com  <AutoShape>  [Misc]
SUBCKT OPT201KP/BB     Com In- V+ V- Out Rfb  <AutoShape>  [Misc]
SUBCKT OPAMP/BB        Unresolved pinout 5 terminals  [-]
SUBCKT OPT202/BB       Com In- V+ V- Out Rfb  <AutoShape>  [Misc]
SUBCKT OPAMP/BB_R_1    Unresolved pinout 5 terminals  [-]
SUBCKT OPT209/BB       Com In- V+ V- Out Rfb  <AutoShape>  [Misc]
SUBCKT OPAMP/BB_R_2    Unresolved pinout 5 terminals  [-]
SUBCKT OPT211/BB       Com In- V+ V- Out Photo  <AutoShape>  [Misc]
SUBCKT OPAMP/BB_R_3    Unresolved pinout 5 terminals  [-]
SUBCKT OPT301/BB       Com In- V+ V- Out Rfb  <AutoShape>  [Misc]
SUBCKT OPAMP/BB_R_4    Unresolved pinout 5 terminals  [-]
SUBCKT PGA206/BB       VO1 In- In+ V- VO2 Ref VO Sense V+ DigGnd A0 A1  <AutoShape>  [Misc]
SUBCKT AND/BB          Unresolved pinout 4 terminals  [-]
SUBCKT XOR/BB          Unresolved pinout 4 terminals  [-]
SUBCKT NOR/BB          Unresolved pinout 5 terminals  [-]
SUBCKT OPAMP/BB_R_5    In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT PGA207/BB       VO1 In- In+ V- VO2 Ref VO Sense V+ DigGnd A0 A1  <AutoShape>  [Misc]
SUBCKT AND/BB_R_1      Unresolved pinout 4 terminals  [-]
SUBCKT XOR/BB_R_1      Unresolved pinout 4 terminals  [-]
SUBCKT NOR/BB_R_1      Unresolved pinout 5 terminals  [-]
SUBCKT OPAMP/BB_R_6    In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT RCV/BB          Unresolved pinout 14 terminals  [-]
SUBCKT UAF42/BB        OutL In3 In2 In+Aux In-Aux OutAux OutB FreqAdj1 V- V+ Gnd In1 OutH FreqAdj2  <AutoShape>  [OpAmp]
SUBCKT AMP_UAF/BB      In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT UAF42E/BB       OutL In3 In2 In+Aux In-Aux OutAux OutB FreqAdj1 V- V+ Gnd In1 OutH FreqAdj2  <AutoShape>  [OpAmp]
SUBCKT AMP_UAFE/BB     In+ In- V+ V- Out  <Amplifier5> [OpAmp]
SUBCKT VCA610M/BB      In+ Q1=Gnd Q2=Gain Out V+ V- In-  <Amplifier7> [OpAmp]
